[bookmark: _GoBack]Provide and install a Back Pressure Regulating Valve as shown on the contract drawings.  The valve shall be a 1" NPT Preferred Utilities Manufacturing Corporation, Danbury, CT, Model V.  The valve shall be diaphragm operated with 250 lb cast iron body, hardened stainless steel trim with an adjustable spring range from _____ to _____ psig.
