[bookmark: _GoBack]Provide and install at the bottom of the tank suction a double poppet foot valve of bronze construction, with lapped-in seats, flat poppets and 20 mesh monel screen. The valve shall be a Preferred Utilities Mfg. Corp., Danbury, CT, Model 22 (add -2 for 2" size) Double Poppet Foot Valves.
