[bookmark: _GoBack]Provide and mount a dial pressure gauge on the discharge side of each pump. Gauges should be selected to provide mid-scale readings under normal operating pressures. Gauges shall be liquid filled to dampen pulsation, with bright finished stainless steel case, brass movement, bronze Bourdon tube, and shall be furnished with a pulsation dampening orifice. Gauges shall be mounted with isolation cocks.  Each gauge shall be equipped with an isolation ball valve. Pressure Gauge shall be furnished by Preferred Utilities Mfg. Corp., Danbury, CT.  
