Furnish and install where shown one _____" threaded duplex fuel oil strainer. Diverting of the strainer handle shall allow for maintenance of dirty basket without interruption of flow. Strainer shall have one piece cast ductile iron 60 body (ASTM A-536) and shall be hydrostatically tested to U.L. quality control specifications. Strainer shall be compatible with the following fluids: #2 Diesel, Biodiesels up to B100, and Renewable Diesel up to R100. The strainer baskets shall be constructed of 5/32" perforated and (40) (60) (100) mesh stainless steel. Strainer shall be Preferred Utilities Mfg. Corp., Danbury, CT, Model DPS.
