[bookmark: _GoBack]Provide and mount a dial thermometer at the inlet and outlet of each heater. Gauge shall have a 2" white dial with a stainless steel, hermetically sealed construction, and matching thermowell. Gauge shall be calibrated from 50º to +300º F and be furnished by Preferred Utilities Manufacturing Corporation, Danbury, CT, Oil Thermometer.
