[bookmark: _GoBack]All expansion and pressure relief valves shall be sized and located as shown on project drawings.  Valve bodies shall be one piece bronze construction suitable for pressures up to 300 psig.  Valves shall be Model R as furnished by Preferred Utilities Manufacturing Corporation, Danbury, CT, with an adjustable range from  ______ to ______ psig.
