[bookmark: _GoBack]Oil strainers shall have cast iron body, with threaded connections, sized as shown on the drawings and suitable for working pressures to 200 psig. Clamped cover and handle shall permit easy removal of the basket. Basket shall be constructed of (3/64" perforated) (40 mesh) (100 mesh) stainless steel. Strainer shall be Preferred Utilities Manufacturing Corporation, Danbury, CT, Model 125.
