[bookmark: _GoBack]Each storage tank fill and sounding line shall terminate in a galvanized, cast iron fill body with threaded brass cap and oil-treated gasket to make it watertight.  Assembly shall be the full size of the pipe and shall be a Preferred Utilities Manufacturing Corporation, Danbury, CT,  Model W.
