[bookmark: _GoBack]Provide and install an Overfill Caution Sign near the Overfill Alarm Station. The sign shall be 20"W by 14"H of 18 gauge steel with porcelain baked enamel finished bright yellow background and minimum 2"H black lettering. The Caution Sign shall read: CAUTION WHEN ALARM BELL SOUNDS OIL TANK FILLED TO CAPACITY DO NOT OVERFILL. Sign shall be a Preferred Utilities Manufacturing Corporation, Danbury, CT, Fil-Alarm Sign Model FA-S.
