[bookmark: _GoBack]Provide and install where shown on the drawings an Audible/ Visual Overfill Alarm Station for (1, 2, or 3) tanks to be activated by Preferred Utilities HLS high level switch, TG-ELD4A Tank Gauges. The system shall consist of a Preferred FA-S caution sign and stainless steel NEMA 4X rated moisture-proof and corrosion-proof enclosure, including a 6" weather-proof bell with automatic silencing, 180° visible flashing lamp, bell silencing push button, and alarm test push button. Overfill alarm station shall be a Preferred Utilities Mfg. Corp., Danbury, CT, Model FA-AV-SS. To add gallons display to FA-AV-SS add: "to include a digital display of tank content, reading directly in gallons without multiplier."
