[bookmark: _GoBack]Furnish and install where shown on contract drawings a quick-closing, spring-loaded and thermally-actuated fusible element that melts at 165° F causing the valve to close tightly. The valve shall be a Preferred Utilities Mfg. Corp., Danbury, CT, Fusomatic Valve.
