[bookmark: _GoBack]Fuel oil storage Tank Vent Protector shall be the full size of the vent pipe or in accordance with NFPA 30 2-4.5.2. It shall be of aluminum construction and provided with standard pipe threads. A standard Tank Vent Protector must be furnished by Preferred Utilities Mfg. Corp., Danbury, CT.
