[bookmark: _GoBack]Provide where shown on the drawings a switch for leak sensing on all containment piping within the building. There shall be a switch at the end of each pitched horizontal run.  Switches shall integrate with fuel oil management control center. The Leak Detection Switch shall be Preferred Utilities Mfg. Corp., Danbury, CT, Model RBS. 
